December 28, 2017

RE: Roof Hatch Safety Railing Product Change Notice

Nystrom announces the release of our updated Roof Hatch Safety Railing in aluminum.

Additions to the design:

* + New Aluminum rail and gate construction
	+ Light weight design allows for easier and faster installation
	+ Meets OSHA 29 CFR 1926.502
	+ Available in standard and custom sizes, fits all brands of roof hatches that have a counterflash
	+ Powder coat finish options available, including safety yellow
	+ Still provides a non-penetrating attachment to the hatch via the counterflash
	+ 5 year warranty

Specifications:

* + Rails / Posts – Aluminum pipe, 1-1/4 inch (31 mm), schedule 40, 6061 T6 alloy
	+ Fittings – Aluminum alloy 5052-H32
	+ Gate – Aluminum pipe, 1-1/4 inch (31 mm), schedule 40, 6061 T6 alloy
	+ Mounting brackets – 3/16 inch steel, zinc plated



The new aluminum safety rail and gate will begin shipping January 15, 2018. Please contact us at 1.800.547.2635 should you have any questions or concerns. We appreciate the opportunity to service you.