**Compression Seal EJ-SES**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **LEED Category** | **Credit** | **Details** | **Possible Points** | **Product/Material Detail** |
| Material and Resources (MR) | 4 | Recycled Content: Post-consumer and Pre-consumer content | 1 to 2 possible points | Seals contain 0% pre-consumer and 0% post-consumer recycled content. |
| 5 | Regional Material: Use building materials or products that have been extracted, harvested or recovered, as well as manufactured,  within 500 miles of the project site | 1 to 2 possible points | Not applicable. Extraction point is not within 500 miles of manufacturing.  Final Packaging Facility Location |
| Indoor Environmental Quality (IEQ) | 4.3 | Low Emitting Materials (Adhesives and Sealants): All sealants must meet the requirements of IEQ 4.1: Adhesives and Sealants, which includes a volatile organic compound (VOC) limit of 50 g/L. | 1 possible point | The VOC of the silicone used in Nystrom SES is approximately 39 grams / liter |