

1. Frame the opening



3. Mount frame into place



5. Tape and apply drywall compound

### Model(s): GFR



2. Mount Seamless™ surround with drywall screws



4. Install drywall and place access panel in opening



6. Apply desired finish