­

May 2017

Re: Potential LEED credits for projects (based on LEED-NC, version 2.1)

To whom it may concern:

Nystrom certifies and provides the following information for use in achieving LEED-NC credit for the specification of Nystrom Expansion Joint Systems.

Products: **Exterior Expansion Joint; All Weather Seal**

Model(s): **EW**

**MR Credits 4.1 & 4.2:**

Recycled Content In figuring recycled content, we use the default value of 25% post-consumer recycled content for the metal and components. Total recycled content by weight for the assembly is equal to 25% post-consumer Recycled content.

**MR Credit 5.1: Regional Materials**

Materials are not extracted within 500 miles of manufacturing plant.

**EQ Credit 4.1: Low-Emitting Materials, Adhesives & Sealants**

Not applicable. Product does not require adhesives or sealants in the field.

**EQ Credit 4.2 Low-Emitting Materials, Paints & Coatings**

Not applicable. All paints and coatings are applied at the factory.

Note - No building products are LEED certified; only buildings are certified. Building products can only contribute to earning points in various categories.

If you require any further information, please do not hesitate to contact us.