­

May 2017

Re: Potential LEED credits for projects (based on LEED-NC, version 2.1)

To whom it may concern:

Nystrom certifies and provides the following information for use in achieving LEED-NC credit for the specification of Nystrom Expansion Joint Systems.

Products: **Seismic Security Exterior Wall System**

Model(s): **RJX**

**MR Credits 4.1 & 4.2 Recycled Content**

This product is made from 6063 T6 aluminum alloy, with zinc plated steel hardware. In figuring recycled content, we use the default value of 25% post-consumer recycled content for the metal and components. Total recycled content by weight for the assembly is equal to 25% post-consumer recycled content.

**MR Credit 5.1 Regional Materials**

Materials are not extracted within 500 miles of manufacturing plant.

**EQ Credit 4.1, Adhesives and Sealants**

Not applicable. Product does not require adhesives or sealants in the field.

**EQ Credit 4.2 Low-emitting Materials, Paints and Coatings**

Not applicable. All paints and coatings are applied at the factory.

If you require any further information, please do not hesitate to contact us.