­

May 2017

Re: Potential LEED credits for projects (based on LEED-NC, version 2.1)

To whom it may concern:

Nystrom certifies and provides the following information for use in achieving LEED-NC credit for the specification of Nystrom Wall and Door Protection.

Product: **Stainless Steel Corner Guards, Crash Rails and Wall Covering**

Model(s): **CGSS, CRS, WCS**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| LEED Category | Credit | Details | Points | Product/Material Detail |
| Material and Resource  (MR) | 4 | Recycled Content: Post-consumer +1/2  Pre-consumer content | 1 to 2  possible points | Corner Guards:   * Contains 70% pre-consumer and 0% post-consumer recycled content.   Extended Mount Crash Rails:   * Contains 69% pre-consumer and 0% post-recycled content.   Surface Mount Crash Rails:   * Contains 38% pre-consumer and 0% post-consumer recycled content.   Stainless Steel Wall Covering:   * Contains 70% pre-consumer and 0% post-consumer recycled content. |
| 5 | Regional material: Use building materials or products that have been extracted, harvested or recovered, as well as manufactured, within 500 miles of the project site | 1 to 2  possible points | Not applicable. Extraction point is not within 500 miles of manufacturing.  Extraction Point is:   * Outside USA   Final Packaging Facility Location:   * Brooklyn Park, MN |

If you require any further information, please do not hesitate to contact us.­